IFC building model
Schema: "IFC4X1"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Y:\\Publikationen\\2022_RSA_BIM\\supplementary_material\\BIMGM.ifc"
Time stamp: "2022-02-01T13:35:31"
Author: "Undefined"
Organization: "Undefined"
Preprocessor: "BricsCAD BIM 22.1.06"
Originating system: "BricsCAD BIM 22.1.06"
Authorization: "Undefined"
Application: "BricsCAD Civil" version "V22" identifier "Bcad" by Organization "Bricsys nv"

People and organizations
  Person "Bricsys" of Organization "Bricsys nv"
  Owner history of Person "Bricsys" of Organization "Bricsys nv" | application "BricsCAD Civil" version "V22" identifier "Bcad" by Organization "Bricsys nv" | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: RADIAN
  TIMEUNIT: SECOND
  MASSUNIT: GRAM

Spatial structure
IFCPROJECT "BIMGM"
  IFCSITE "Site" | latitude 37° 47′ 42″ | longitude -122° 23′ 38.4″ | elevation above sea level 0.
    IFCBUILDING "Geotechnical model" | reference height above sea level 0. | terrain above sea level 0.
      IFCBUILDINGSTOREY "Geotechnical Unit" | elevation 0.
        contains 5 elements
          5 x IFCBUILDINGELEMENTPROXY | names: "Sediment cover", "Unterangerberg Formation weathered", "Unterangerberg Formation" (+1 more) | property sets: PSet_GeologyGeneral, PSet_GeotechUnits
      IFCBUILDINGSTOREY "Cross section" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | names: "Crosssection 1" | property sets: PSet_CrossSection
    IFCBUILDING "Geotechnical synthesis model" | reference height above sea level 0. | terrain above sea level 0.
      IFCBUILDINGSTOREY "GSM_Geology" | elevation 0.
        contains 3 elements
          3 x IFCBUILDINGELEMENTPROXY | names: "Damage Zone of the Unterangerberg Formation", "Unterangerberg Formation" | property sets: PSet_GeologyGeneral, PSet_GeotechUnits, PSet_Phenomena, PSet_Semantics_General
    IFCBUILDING "Factual data model" | reference height above sea level 0. | terrain above sea level 0.
      IFCBUILDINGSTOREY "Boring" | elevation 0.
        contains 2 elements
          2 x IFCBUILDINGELEMENTPROXY | names: "A-KB 02/21", "A-KB 01/21" | property sets: PSet_Borehole

Property sets
  PSet_GeologyGeneral | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    GeologicalUnits = "Unterangerberg Formation" (IFCTEXT)
  PSet_GeologyGeneral | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    GeologicalUnits = "Damage Zone of the Unterangerberg Formation" (IFCTEXT)
  PSet_GeologyGeneral | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    GeologicalUnits = "Sediment cover" (IFCTEXT)
  PSet_GeologyGeneral | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    GeologicalUnits = "Unterangerberg Formation weathered" (IFCTEXT)
  PSet_GeotechUnits | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    GeotechUnit_1 = "1" (IFCTEXT)
    GeotechUnit_1_Description = "Marl of the Unterangerberg Formation, fresh to slightly weathered" (IFCTEXT)
    GeotechUnit_1_Parameter = "\Linked_Data_Sheet\Rockmass_1.pdf" (IFCTEXT)
    GeotechUnit_1_Percent = 80. (IFCREAL)
    GeotechUnit_2 = "2" (IFCTEXT)
    GeotechUnit_2_Description = "Marl of the Unterangerberg Formation, slightly weathered" (IFCTEXT)
    GeotechUnit_2_Parameter = "\Linked_Data_Sheet\Rockmass_2.pdf" (IFCTEXT)
    GeotechUnit_2_Percent = 20. (IFCREAL)
  PSet_GeotechUnits | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    GeotechUnit_1 = "1" (IFCTEXT)
    GeotechUnit_1_Description = "Marl of the Unterangerberg Formation, fresh to slightly weathered" (IFCTEXT)
    GeotechUnit_1_Parameter = "\Linked_Data_Sheet\Rockmass_1.pdf" (IFCTEXT)
    GeotechUnit_1_Percent = 85. (IFCREAL)
    GeotechUnit_2 = "3" (IFCTEXT)
    GeotechUnit_2_Description = "Damage Zone" (IFCTEXT)
    GeotechUnit_2_Parameter = "\Linked_Data_Sheet\Rockmass_3.pdf" (IFCTEXT)
    GeotechUnit_2_Percent = 15. (IFCREAL)
  PSet_GeotechUnits | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    GeotechUnit_1 = "4" (IFCTEXT)
    GeotechUnit_1_Description = "Sediments" (IFCTEXT)
    GeotechUnit_1_Parameter = "\Linked_Data_Sheet\Rockmass_4.pdf" (IFCTEXT)
    GeotechUnit_1_Percent = 100. (IFCREAL)
  PSet_GeotechUnits | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    GeotechUnit_1 = "1" (IFCTEXT)
    GeotechUnit_1_Description = "Marl of the Unterangerberg Formation, fresh to slightly weathered" (IFCTEXT)
    GeotechUnit_1_Parameter = "\Linked_Data_Sheet\Rockmass_1.pdf" (IFCTEXT)
    GeotechUnit_1_Percent = 100. (IFCREAL)
  PSet_Phenomena | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    OccurenceGas = "" (IFCTEXT)
  PSet_Semantics_General | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    TunnelmeterEnd = 75.43000000000001 (IFCREAL)
    TunnelmeterStart = 29.59000000000000 (IFCREAL)
  PSet_Semantics_General | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    TunnelmeterEnd = 100. (IFCREAL)
    TunnelmeterStart = 75.43000000000001 (IFCREAL)
  PSet_Semantics_General | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    TunnelmeterEnd = 29.59000000000000 (IFCREAL)
  PSet_Borehole | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    DrillingCompany = "ExampleComp" (IFCTEXT)
    DrillingEnd = "20.12.2020" (IFCTEXT)
    DrillingStart = "20.12.2020" (IFCTEXT)
    DrillogRel = "\Linked_Drill_Logs\A-KB_01-21\A-KB_02-21.pdf" (IFCTEXT)
    MaxWaterHeightAbsolute = 123.1200000000000 (IFCREAL)
    MaxWaterHeightDate = "20.12.2020" (IFCTEXT)
    MinWaterHeightAbsolute = 121.3400000000000 (IFCREAL)
    MinWaterheightDate = "20.12.2020" (IFCTEXT)
    Name = "A-KB 02/21" (IFCTEXT)
    ObservationPeriodEnd = "20.12.2020" (IFCTEXT)
    ObservationPeriodStart = "20.12.2020" (IFCTEXT)
    WellType = "refilled" (IFCTEXT)
  PSet_Borehole | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    DrillingCompany = "ExampleComp" (IFCTEXT)
    DrillingEnd = "20.12.2020" (IFCTEXT)
    DrillingStart = "20.12.2020" (IFCTEXT)
    DrillogRel = "\Linked_Drill_Logs\A-KB_01-21\A-KB_01-21.pdf" (IFCTEXT)
    MaxWaterHeightAbsolute = 123.8500000000000 (IFCREAL)
    MaxWaterHeightDate = "20.12.2020" (IFCTEXT)
    MinWaterHeightAbsolute = 121.3200000000000 (IFCREAL)
    MinWaterheightDate = "20.12.2020" (IFCTEXT)
    Name = "A-KB 01/21" (IFCTEXT)
    ObservationPeriodEnd = "20.12.2020" (IFCTEXT)
    ObservationPeriodStart = "20.12.2020" (IFCTEXT)
    WellType = "refilled" (IFCTEXT)
  PSet_CrossSection | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    CrossSectionName = "Crosssection 1" (IFCTEXT)
    CrossSectionRel = "\Linked_Cross_Sections\Cross_Section_1.pdf" (IFCTEXT)